Corn fest mini rod rules

SMALL TIRE CLASS 1850 lb 1900 lb 34in TIRES OR LESS

BIG TIRE CLASS 1950lb 18.4 x 16.1 OR LESS TIRES

1 All mini rods are required to use automotive engines only 420 cubic in or less

2 No portion of any mini rod may exceed 8 feet forward from the center of the rear axle to front most point

3 The width of the mini rod may not exceed 6 feet from the edge of the tire tread to edge of tire tread

4 All power will be transmitted though the rear wheels of the mini rod

5 All mini rods are required to have wide front ends with two wheels . The front wheels must track within any portion of the rear wheels

6 All exhaust pipes must be projected upward

7 All mini rods are required to have SAFETY KILL SWITCH and NEUTRAL START SWITCH

8 All mini rods are required to have skid pads

9 All mini rods must have rear brakes that must be operated by foot and must be able to stop machine

10 Engines require side plates that go along the length of the block and up to the bottom of the head 1/8 in aluminum or 1/16 in steel is the minimum

11 Engines are required to have damper pulley shielded 360 degrees with a strap across the front that is all no less then 1/8 in thick and 1in wide blow proof balancer just needs one across front

12 Mini rods running a manual transmission are required to have blow proof bell housing

13 Mini rods running automatic transmission are required a SFI safety blanket or SFI approved shield

14 All open chains and or drive shafts need to be shielded 180 degrees top and sides must be 1/8 thickness

15 All open fans must be shielded across top and down both sides at least 1/16 thick metal

16 Hand throttles or foot feed If hand throttle it must push forward and when released must return to idle on its own

17 mini rods must have roll cage

18 mini rods must have seat belts

19 Mini rods must have fenders

20 All engines must be naturally aspirated NO blowers or turbo

21 No nitrous oxide

22 Maximum drawbar height is 13 inches

23 Fire suits are required for all drivers

24 When mini rod is running driver must be sitting in drivers seat

25 Driver can pull up to the 75 foot mark before stopping trying again this rule does not apply in a pull off

26 First puller after eliminator IS SET will be first puller in that class This puller has option to take this pull or drop to last if driver opts to repull the second pull is measured Decision to take or leave the first pull must be made before mini rod leaves track

27 Any part of mini rod going out of bounds on first pull is DISQUALIFIED [Out of bounds is any portion of mini rod touching the line or breaking the plan of the line] on pull-off it is point or measure

28 Anything FALLING OFF mini rod will DISQUALIFY mini rod for that class In a pull-off mini rod drops to bottom of others in pull-off

29 NO ALCOHOL AT ALL ALLOWED ON THE TRACK no drinking by drivers until finished pulling for the day